From an Assembly Language point-of-view, any registers that are touched by a function need to be preserved and restored to their original value when that function ends its execution.

Each machine language instruction typically matches a specific CPU instruction from the CPU's instruction set.